Setting up DNS (BIND) 4.9.6

Scenario 1 

Hosting Type 

: Single Domain

Domain 

: skokie.com.sg

IP Range 

: 202.42.220.0 – 202.42.220.255

DNS Server Function : Primary DNS

Secondary DNS 
: secdns.pacific.net.sg

Gateway 


: gw.skokie.com.sg 
- 202.42.220.1

Name Server


: ns.skokie.com.sg
- 202.42.220.5

Web Server


: www.skokie.com.sg
- 202.42.220.15

Mail Server


: mail.skokie.com.sg
- 202.42.220.20

Secondary Mail Server
: po.skokie.com.sg
- 202.42.220.21

named.boot File

;

;    File:       named.boot

;    Purpose:    give the DNS its startup parameters and

;                list of startup files.

Directory c:\\bind

;

;check-names primary fail

;check-names secondary warn

;check-names response ignore

;

;

;    establish a loopback entry for this machine, and tell

;    it to load its identity from db.127.0.0

primary 0.0.127.IN-ADDR.ARPA db.127.0.0

;    XFRNETS parameter limits the transfer of zone information

;    to machines matching the subnet wildcard/mask entries listed.

;    WARNING: I have also added myself so that I can help test out

;             peoples configs that are having problems.

XFRNETS 199.72.93.0 127.0.0.0 202.42.220.0

;    set ourselves as primary server for the zone

primary skokie.com.sg db.zoneinfo

;    provide reverse address-to-host mapping

primary 220.42.202.in-addr.arpa db.202.42.220.0

;

; prime the DNS with root server 'hint' information

cache . db.cache

db.zoneinfo File

;

;    File:      db.zoneinfo

;    Purpose:   This file establishes the name/address information

;               for this zone.  You will have to fill out the actual

;               information for your specific zone in the format shown

;               in the comments.

;

@        IN SOA    ns.skokie.com.sg. postmaster.skokie.com.sg. (

        1997121901   ; serial  [yyyyMMddNN]

             21600   ; refresh [6h]

              3600   ; retry   [1h]

            691200   ; expire  [8d]

             86400)  ; minimum [1d]

skokie.com.sg
IN 
NS  
ns.skokie.com.sg. 




IN
NS
secdns.pacific.net.sg.

skokie.com.sg
IN
MX
10 mail.skokie.com.sg.




IN
A
202.42.220.20




IN
MX
20 po.skokie.com.sg.




IN
A
202.42.220.21

;
Define local hosts    

gw


IN
A
202.42.220.1

ns     

IN    A   
202.42.220.5

www


IN
A
202.42.220.15

mail


IN
A
202.42.220.20

po


IN
A
202.42.220.21

db.202.42.220.0 File

;

;    File:      db.inaddr

;    Purpose:   This file establishes the address-to-name lookup

;               information for this zone.  You will have to

;               fill out the actual address information for your

;               specific zone in the format shown in the comments

;

@        IN SOA ns.skokie.com.sg. postmaster.skokie.com.sg. (

        1997121901   ; serial  [yyyyMMddNN]

             21600   ; refresh [6h]

              3600   ; retry   [1h]

            691200   ; expire  [8d]

             86400)  ; minimum [1d]

   
IN 
NS 
ns.skokie.com.sg. 


IN
NS
secdns.pacific.net.sg.

1        
IN 
PTR   gw.skokie.com.sg.

5       
IN 
PTR  
ns.skokie.com.sg.

15

IN
PTR
www.skokie.com.sg.

20

IN
PTR
mail.skokie.com.sg.

21

IN
PTR
po.skokie.com.sg.

db.127.0.0 File

;

;    File:      db.127.0.0 file

;    Purpose:   This file establishes the identity of this DNS.

;               SOA stands for 'start of authority' and sets the

;               default parameters for information this DNS is 

;               authoritative for:

;

@        IN SOA    ns.skokie.com.sg. postmaster.skokie.com.sg. (

        1997121901   ; serial  [yyyyMMddNN]

             21600   ; refresh [6h]

              3600   ; retry   [1h]

            691200   ; expire  [8d]

             86400)  ; minimum [1d]

;

         
IN 
NS 
ns.skokie.com.sg. 



IN
NS
secdns.pacific.net.sg.

1        
IN 
PTR   localhost.skokie.com.sg.

;

Scenario 2

Hosting Type 

: Multiple Domains for Web Hosting Only

Domains 

: skokie.com.sg




  ohare.com.sg




  palatine.com.sg

IP Range 

: 202.42.220.0 – 202.42.220.255

DNS Server Function : Primary DNS

Secondary DNS 
: secdns.pacific.net.sg

Gateway 


: gw.skokie.com.sg 
- 202.42.220.1

Name Server


: ns.skokie.com.sg
- 202.42.220.5

Web Server


: www.skokie.com.sg
- 202.42.220.15

Mail Server


: mail.skokie.com.sg
- 202.42.220.20

Secondary Mail Server
: po.skokie.com.sg
- 202.42.220.21

Web Server – Ohare

: www.ohare.com.sg
- 202.42.220.30

Web Server – palatine

: www.palatine.com.sg - 202.42.220.31

named.boot File

;

;    File:       named.boot

;    Purpose:    give the DNS its startup parameters and

;                list of startup files.

Directory c:\\bind

;

;check-names primary fail

;check-names secondary warn

;check-names response ignore

;

;

;    establish a loopback entry for this machine, and tell

;    it to load its identity from db.127.0.0

primary 0.0.127.IN-ADDR.ARPA db.127.0.0

;    XFRNETS parameter limits the transfer of zone information

;    to machines matching the subnet wildcard/mask entries listed.

;    WARNING: I have also added myself so that I can help test out

;             peoples configs that are having problems.

XFRNETS 199.72.93.0 127.0.0.0 202.42.220.0

;    set ourselves as primary server for the zone

primary skokie.com.sg db.zoneinfo

primary ohare.com.sg db.ohare

primary palatine.com.sg db.palatine

;    provide reverse address-to-host mapping

primary 220.42.202.in-addr.arpa db.202.42.220.0

;

; prime the DNS with root server 'hint' information

cache . db.cache

db.zoneinfo File

;

;    File:      db.zoneinfo

;    Purpose:   This file establishes the name/address information

;               for this zone.  You will have to fill out the actual

;               information for your specific zone in the format shown

;               in the comments.

;

@        IN SOA    ns.skokie.com.sg. postmaster.skokie.com.sg. (

        1997121901   ; serial  [yyyyMMddNN]

             21600   ; refresh [6h]

              3600   ; retry   [1h]

            691200   ; expire  [8d]

             86400)  ; minimum [1d]

skokie.com.sg
IN 
NS  
ns.skokie.com.sg. 




IN
NS
secdns.pacific.net.sg.

skokie.com.sg
IN
MX
10 mail.skokie.com.sg.




IN
A
202.42.220.20




IN
MX
20 po.skokie.com.sg.




IN
A
202.42.220.21

;
Define local hosts    

gw


IN
A
202.42.220.1

ns     

IN    A   
202.42.220.5

www


IN
A
202.42.220.15

mail


IN
A
202.42.220.20

po


IN
A
202.42.220.21

db.ohare File

;

;    File:      db.ohare

;    Purpose:   This file establishes the name/address information

;               for this zone.  You will have to fill out the actual

;               information for your specific zone in the format shown

;               in the comments.

;

@        IN SOA    ns.skokie.com.sg. postmaster.skokie.com.sg. (

        1997121901   ; serial  [yyyyMMddNN]

             21600   ; refresh [6h]

              3600   ; retry   [1h]

            691200   ; expire  [8d]

             86400)  ; minimum [1d]

ohare.com.sg
IN 
NS  
ns.skokie.com.sg. 




IN
NS
secdns.pacific.net.sg.

;
Define local hosts    

www


IN
A
202.42.220.30

db.palatine File

;

;    File:      db.palatine

;    Purpose:   This file establishes the name/address information

;               for this zone.  You will have to fill out the actual

;               information for your specific zone in the format shown

;               in the comments.

;

@        IN SOA    ns.skokie.com.sg. postmaster.skokie.com.sg. (

        1997121901   ; serial  [yyyyMMddNN]

             21600   ; refresh [6h]

              3600   ; retry   [1h]

            691200   ; expire  [8d]

             86400)  ; minimum [1d]

palatine.com.sg
IN 
NS  
ns.skokie.com.sg. 




IN
NS
secdns.pacific.net.sg.

;
Define local hosts    

www


IN
A
202.42.220.31

db.202.42.220.0 File

;

;    File:      db.inaddr

;    Purpose:   This file establishes the address-to-name lookup

;               information for this zone.  You will have to

;               fill out the actual address information for your

;               specific zone in the format shown in the comments

;

@        IN SOA ns.skokie.com.sg. postmaster.skokie.com.sg. (

        1997121901   ; serial  [yyyyMMddNN]

             21600   ; refresh [6h]

              3600   ; retry   [1h]

            691200   ; expire  [8d]

             86400)  ; minimum [1d]

   
IN 
NS 
ns.skokie.com.sg. 


IN
NS
secdns.pacific.net.sg.

1        
IN 
PTR   gw.skokie.com.sg.

5       
IN 
PTR  
ns.skokie.com.sg.

15

IN
PTR
www.skokie.com.sg.

20

IN
PTR
mail.skokie.com.sg.

21

IN
PTR
po.skokie.com.sg.

30

IN
PTR
www.ohare.com.sg.

31

IN
PTR
www.palatine.com.sg.

db.127.0.0 File

;

;    File:      db.127.0.0 file

;    Purpose:   This file establishes the identity of this DNS.

;               SOA stands for 'start of authority' and sets the

;               default parameters for information this DNS is 

;               authoritative for:

;

@        IN SOA    ns.skokie.com.sg. postmaster.skokie.com.sg. (

        1997121901   ; serial  [yyyyMMddNN]

             21600   ; refresh [6h]

              3600   ; retry   [1h]

            691200   ; expire  [8d]

             86400)  ; minimum [1d]

;

         
IN 
NS 
ns.skokie.com.sg. 



IN
NS
secdns.pacific.net.sg.

1        
IN 
PTR   localhost.skokie.com.sg.

;

Scenario 3

Hosting Type 

: Multiple Domains for Web Hosting & Mail Server




  Mail Servers on separate hosts

Domains 

: skokie.com.sg




  ohare.com.sg




  palatine.com.sg

IP Range 

: 202.42.220.0 – 202.42.220.255

DNS Server Function : Primary DNS

Secondary DNS 
: secdns.pacific.net.sg

Gateway 


: gw.skokie.com.sg 
- 202.42.220.1

Name Server


: ns.skokie.com.sg
- 202.42.220.5

Web Server


: www.skokie.com.sg
- 202.42.220.15

Mail Server


: mail.skokie.com.sg
- 202.42.220.20

Secondary Mail Server
: po.skokie.com.sg
- 202.42.220.21

Web Server – Ohare

: www.ohare.com.sg
- 202.42.220.30

Web Server – palatine

: www.palatine.com.sg - 202.42.220.31

Mail Server – Ohare

: mail.ohare.com.sg 
- 202.42.220.40

Mail Server – palatine

: mail.palatine.com.sg
- 202.42.220.41

named.boot File

;

;    File:       named.boot

;    Purpose:    give the DNS its startup parameters and

;                list of startup files.

Directory c:\\bind

;

;check-names primary fail

;check-names secondary warn

;check-names response ignore

;

;

;    establish a loopback entry for this machine, and tell

;    it to load its identity from db.127.0.0

primary 0.0.127.IN-ADDR.ARPA db.127.0.0

;    XFRNETS parameter limits the transfer of zone information

;    to machines matching the subnet wildcard/mask entries listed.

;    WARNING: I have also added myself so that I can help test out

;             peoples configs that are having problems.

XFRNETS 199.72.93.0 127.0.0.0 202.42.220.0

;    set ourselves as primary server for the zone

primary skokie.com.sg db.zoneinfo

primary ohare.com.sg db.ohare

primary palatine.com.sg db.palatine

;    provide reverse address-to-host mapping

primary 220.42.202.in-addr.arpa db.202.42.220.0

;

; prime the DNS with root server 'hint' information

cache . db.cache

db.zoneinfo File

;

;    File:      db.zoneinfo

;    Purpose:   This file establishes the name/address information

;               for this zone.  You will have to fill out the actual

;               information for your specific zone in the format shown

;               in the comments.

;

@        IN SOA    ns.skokie.com.sg. postmaster.skokie.com.sg. (

        1997121901   ; serial  [yyyyMMddNN]

             21600   ; refresh [6h]

              3600   ; retry   [1h]

            691200   ; expire  [8d]

             86400)  ; minimum [1d]

skokie.com.sg
IN 
NS  
ns.skokie.com.sg. 




IN
NS
secdns.pacific.net.sg.

skokie.com.sg
IN
MX
10 mail.skokie.com.sg.




IN
A
202.42.220.20




IN
MX
20 po.skokie.com.sg.




IN
A
202.42.220.21

;
Define local hosts    

gw


IN
A
202.42.220.1

ns     

IN    A   
202.42.220.5

www


IN
A
202.42.220.15

mail


IN
A
202.42.220.20

po


IN
A
202.42.220.21

db.ohare File

;

;    File:      db.ohare

;    Purpose:   This file establishes the name/address information

;               for this zone.  You will have to fill out the actual

;               information for your specific zone in the format shown

;               in the comments.

;

@        IN SOA    ns.skokie.com.sg. postmaster.skokie.com.sg. (

        1997121901   ; serial  [yyyyMMddNN]

             21600   ; refresh [6h]

              3600   ; retry   [1h]

            691200   ; expire  [8d]

             86400)  ; minimum [1d]

ohare.com.sg
IN 
NS  
ns.skokie.com.sg. 




IN
NS
secdns.pacific.net.sg.

ohare.com.sg
IN
MX
10 mail.ohare.com.sg.




IN
A
202.42.220.40

;
Define local hosts    

www


IN
A
202.42.220.30

mail


IN
A
202.42.220.40

db.palatine File

;

;    File:      db.palatine

;    Purpose:   This file establishes the name/address information

;               for this zone.  You will have to fill out the actual

;               information for your specific zone in the format shown

;               in the comments.

;

@        IN SOA    ns.skokie.com.sg. postmaster.skokie.com.sg. (

        1997121901   ; serial  [yyyyMMddNN]

             21600   ; refresh [6h]

              3600   ; retry   [1h]

            691200   ; expire  [8d]

             86400)  ; minimum [1d]

palatine.com.sg
IN 
NS  
ns.skokie.com.sg. 




IN
NS
secdns.pacific.net.sg.

palatine.com.sg
IN 
MX  
mail.palatine.com.sg. 




IN
A
202.42.220.41

;
Define local hosts    

www


IN
A
202.42.220.31

mail


IN
A
202.42.220.41

db.202.42.220.0 File

;

;    File:      db.inaddr

;    Purpose:   This file establishes the address-to-name lookup

;               information for this zone.  You will have to

;               fill out the actual address information for your

;               specific zone in the format shown in the comments

;

@        IN SOA ns.skokie.com.sg. postmaster.skokie.com.sg. (

        1997121901   ; serial  [yyyyMMddNN]

             21600   ; refresh [6h]

              3600   ; retry   [1h]

            691200   ; expire  [8d]

             86400)  ; minimum [1d]

   
IN 
NS 
ns.skokie.com.sg. 


IN
NS
secdns.pacific.net.sg.

1        
IN 
PTR   gw.skokie.com.sg.

5       
IN 
PTR  
ns.skokie.com.sg.

15

IN
PTR
www.skokie.com.sg.

20

IN
PTR
mail.skokie.com.sg.

21

IN
PTR
po.skokie.com.sg.

30

IN
PTR
www.ohare.com.sg.

31

IN
PTR
www.palatine.com.sg.

40

IN
PTR
mail.ohare.com.sg.

41

IN
PTR
mail.palatine.com.sg.

db.127.0.0 File

;

;    File:      db.127.0.0 file

;    Purpose:   This file establishes the identity of this DNS.

;               SOA stands for 'start of authority' and sets the

;               default parameters for information this DNS is 

;               authoritative for:

;

@        IN SOA    ns.skokie.com.sg. postmaster.skokie.com.sg. (

        1997121901   ; serial  [yyyyMMddNN]

             21600   ; refresh [6h]

              3600   ; retry   [1h]

            691200   ; expire  [8d]

             86400)  ; minimum [1d]

;

         
IN 
NS 
ns.skokie.com.sg. 



IN
NS
secdns.pacific.net.sg.

1        
IN 
PTR   localhost.skokie.com.sg.

;

Scenario 4

Hosting Type 

: Multiple Domains for Web Hosting & Mail Server




  Mail Servers on ONE single host ONLY

Domains 

: skokie.com.sg




  ohare.com.sg




  palatine.com.sg

IP Range 

: 202.42.220.0 – 202.42.220.255

DNS Server Function : Primary DNS

Secondary DNS 
: secdns.pacific.net.sg

Gateway 


: gw.skokie.com.sg 
- 202.42.220.1

Name Server


: ns.skokie.com.sg
- 202.42.220.5

Web Server


: www.skokie.com.sg
- 202.42.220.15

Mail Server


: mail.skokie.com.sg
- 202.42.220.20

Secondary Mail Server
: po.skokie.com.sg
- 202.42.220.21

Web Server – Ohare

: www.ohare.com.sg
- 202.42.220.30

Web Server – palatine

: www.palatine.com.sg - 202.42.220.31

Mail Server – Ohare

: ohare.com.sg 
- 202.42.220.20

Mail Server – palatine

: palatine.com.sg
- 202.42.220.20

named.boot File

;

;    File:       named.boot

;    Purpose:    give the DNS its startup parameters and

;                list of startup files.

Directory c:\\bind

;

;check-names primary fail

;check-names secondary warn

;check-names response ignore

;

;

;    establish a loopback entry for this machine, and tell

;    it to load its identity from db.127.0.0

primary 0.0.127.IN-ADDR.ARPA db.127.0.0

;    XFRNETS parameter limits the transfer of zone information

;    to machines matching the subnet wildcard/mask entries listed.

;    WARNING: I have also added myself so that I can help test out

;             peoples configs that are having problems.

XFRNETS 199.72.93.0 127.0.0.0 202.42.220.0

;    set ourselves as primary server for the zone

primary skokie.com.sg db.zoneinfo

primary ohare.com.sg db.ohare

primary palatine.com.sg db.palatine

;    provide reverse address-to-host mapping

primary 220.42.202.in-addr.arpa db.202.42.220.0

;

; prime the DNS with root server 'hint' information

cache . db.cache

db.zoneinfo File

;

;    File:      db.zoneinfo

;    Purpose:   This file establishes the name/address information

;               for this zone.  You will have to fill out the actual

;               information for your specific zone in the format shown

;               in the comments.

;

@        IN SOA    ns.skokie.com.sg. postmaster.skokie.com.sg. (

        1997121901   ; serial  [yyyyMMddNN]

             21600   ; refresh [6h]

              3600   ; retry   [1h]

            691200   ; expire  [8d]

             86400)  ; minimum [1d]

skokie.com.sg
IN 
NS  
ns.skokie.com.sg. 




IN
NS
secdns.pacific.net.sg.

skokie.com.sg
IN
MX
10 mail.skokie.com.sg.




IN
A
202.42.220.20




IN
MX
20 po.skokie.com.sg.




IN
A
202.42.220.21

;
Define local hosts    

gw


IN
A
202.42.220.1

ns     

IN    A   
202.42.220.5

www


IN
A
202.42.220.15

mail


IN
A
202.42.220.20

po


IN
A
202.42.220.21

db.ohare File

;

;    File:      db.ohare

;    Purpose:   This file establishes the name/address information

;               for this zone.  You will have to fill out the actual

;               information for your specific zone in the format shown

;               in the comments.

;

@        IN SOA    ns.skokie.com.sg. postmaster.skokie.com.sg. (

        1997121901   ; serial  [yyyyMMddNN]

             21600   ; refresh [6h]

              3600   ; retry   [1h]

            691200   ; expire  [8d]

             86400)  ; minimum [1d]

ohare.com.sg
IN 
NS  
ns.skokie.com.sg. 




IN
NS
secdns.pacific.net.sg.

ohare.com.sg
IN
MX
10 mail.skokie.com.sg.




IN
A
202.42.220.20

;
Define local hosts    

www


IN
A
202.42.220.30

db.palatine File

;

;    File:      db.palatine

;    Purpose:   This file establishes the name/address information

;               for this zone.  You will have to fill out the actual

;               information for your specific zone in the format shown

;               in the comments.

;

@        IN SOA    ns.skokie.com.sg. postmaster.skokie.com.sg. (

        1997121901   ; serial  [yyyyMMddNN]

             21600   ; refresh [6h]

              3600   ; retry   [1h]

            691200   ; expire  [8d]

             86400)  ; minimum [1d]

palatine.com.sg
IN 
NS  
ns.skokie.com.sg. 




IN
NS
secdns.pacific.net.sg.

palatine.com.sg
IN 
MX  
mail.skokie.com.sg. 




IN
A
202.42.220.20

;
Define local hosts    

www


IN
A
202.42.220.31

db.202.42.220.0 File

;

;    File:      db.inaddr

;    Purpose:   This file establishes the address-to-name lookup

;               information for this zone.  You will have to

;               fill out the actual address information for your

;               specific zone in the format shown in the comments

;

@        IN SOA ns.skokie.com.sg. postmaster.skokie.com.sg. (

        1997121901   ; serial  [yyyyMMddNN]

             21600   ; refresh [6h]

              3600   ; retry   [1h]

            691200   ; expire  [8d]

             86400)  ; minimum [1d]

   
IN 
NS 
ns.skokie.com.sg. 


IN
NS
secdns.pacific.net.sg.

1        
IN 
PTR   gw.skokie.com.sg.

5       
IN 
PTR  
ns.skokie.com.sg.

15

IN
PTR
www.skokie.com.sg.

20

IN
PTR
mail.skokie.com.sg.

21

IN
PTR
po.skokie.com.sg.

30

IN
PTR
www.ohare.com.sg.

31

IN
PTR
www.palatine.com.sg.

db.127.0.0 File

;

;    File:      db.127.0.0 file

;    Purpose:   This file establishes the identity of this DNS.

;               SOA stands for 'start of authority' and sets the

;               default parameters for information this DNS is 

;               authoritative for:

;

@        IN SOA    ns.skokie.com.sg. postmaster.skokie.com.sg. (

        1997121901   ; serial  [yyyyMMddNN]

             21600   ; refresh [6h]

              3600   ; retry   [1h]

            691200   ; expire  [8d]

             86400)  ; minimum [1d]

;

         
IN 
NS 
ns.skokie.com.sg. 



IN
NS
secdns.pacific.net.sg.

1        
IN 
PTR   localhost.skokie.com.sg.

;

Scenario 5

Hosting Type 

: Multiple Domains for Mail Only




  Mail Servers on ONE single host ONLY

Domains 

: skokie.com.sg




  ohare.com.sg




  palatine.com.sg

IP Range 

: 202.42.220.0 – 202.42.220.255

DNS Server Function : Primary DNS

Secondary DNS 
: secdns.pacific.net.sg

Gateway 


: gw.skokie.com.sg 
- 202.42.220.1

Name Server


: ns.skokie.com.sg
- 202.42.220.5

Web Server


: www.skokie.com.sg
- 202.42.220.15

Mail Server


: mail.skokie.com.sg
- 202.42.220.20

Secondary Mail Server
: po.skokie.com.sg
- 202.42.220.21

Mail Server – Ohare

: ohare.com.sg 
- 202.42.220.20

Mail Server – palatine

: palatine.com.sg
- 202.42.220.20

named.boot File

;

;    File:       named.boot

;    Purpose:    give the DNS its startup parameters and

;                list of startup files.

Directory c:\\bind

;

;check-names primary fail

;check-names secondary warn

;check-names response ignore

;

;

;    establish a loopback entry for this machine, and tell

;    it to load its identity from db.127.0.0

primary 0.0.127.IN-ADDR.ARPA db.127.0.0

;    XFRNETS parameter limits the transfer of zone information

;    to machines matching the subnet wildcard/mask entries listed.

;    WARNING: I have also added myself so that I can help test out

;             peoples configs that are having problems.

XFRNETS 199.72.93.0 127.0.0.0 202.42.220.0

;    set ourselves as primary server for the zone

primary skokie.com.sg db.zoneinfo

primary ohare.com.sg db.ohare

primary palatine.com.sg db.palatine

;    provide reverse address-to-host mapping

primary 220.42.202.in-addr.arpa db.202.42.220.0

;

; prime the DNS with root server 'hint' information

cache . db.cache

db.zoneinfo File

;

;    File:      db.zoneinfo

;    Purpose:   This file establishes the name/address information

;               for this zone.  You will have to fill out the actual

;               information for your specific zone in the format shown

;               in the comments.

;

@        IN SOA    ns.skokie.com.sg. postmaster.skokie.com.sg. (

        1997121901   ; serial  [yyyyMMddNN]

             21600   ; refresh [6h]

              3600   ; retry   [1h]

            691200   ; expire  [8d]

             86400)  ; minimum [1d]

skokie.com.sg
IN 
NS  
ns.skokie.com.sg. 




IN
NS
secdns.pacific.net.sg.

skokie.com.sg
IN
MX
10 mail.skokie.com.sg.




IN
A
202.42.220.20




IN
MX
20 po.skokie.com.sg.




IN
A
202.42.220.21

;
Define local hosts    

gw


IN
A
202.42.220.1

ns     

IN    A   
202.42.220.5

www


IN
A
202.42.220.15

mail


IN
A
202.42.220.20

po


IN
A
202.42.220.21

db.ohare File

;

;    File:      db.ohare

;    Purpose:   This file establishes the name/address information

;               for this zone.  You will have to fill out the actual

;               information for your specific zone in the format shown

;               in the comments.

;

@        IN SOA    ns.skokie.com.sg. postmaster.skokie.com.sg. (

        1997121901   ; serial  [yyyyMMddNN]

             21600   ; refresh [6h]

              3600   ; retry   [1h]

            691200   ; expire  [8d]

             86400)  ; minimum [1d]

ohare.com.sg
IN 
NS  
ns.skokie.com.sg. 




IN
NS
secdns.pacific.net.sg.

ohare.com.sg
IN
MX
10 mail.skokie.com.sg.




IN
A
202.42.220.20

;
Define local hosts    

db.palatine File

;

;    File:      db.palatine

;    Purpose:   This file establishes the name/address information

;               for this zone.  You will have to fill out the actual

;               information for your specific zone in the format shown

;               in the comments.

;

@        IN SOA    ns.skokie.com.sg. postmaster.skokie.com.sg. (

        1997121901   ; serial  [yyyyMMddNN]

             21600   ; refresh [6h]

              3600   ; retry   [1h]

            691200   ; expire  [8d]

             86400)  ; minimum [1d]

palatine.com.sg
IN 
NS  
ns.skokie.com.sg. 




IN
NS
secdns.pacific.net.sg.

palatine.com.sg
IN 
MX  
mail.skokie.com.sg. 




IN
A
202.42.220.20

;
Define local hosts    

db.202.42.220.0 File

;

;    File:      db.inaddr

;    Purpose:   This file establishes the address-to-name lookup

;               information for this zone.  You will have to

;               fill out the actual address information for your

;               specific zone in the format shown in the comments

;

@        IN SOA ns.skokie.com.sg. postmaster.skokie.com.sg. (

        1997121901   ; serial  [yyyyMMddNN]

             21600   ; refresh [6h]

              3600   ; retry   [1h]

            691200   ; expire  [8d]

             86400)  ; minimum [1d]

   
IN 
NS 
ns.skokie.com.sg. 


IN
NS
secdns.pacific.net.sg.

1        
IN 
PTR   gw.skokie.com.sg.

5       
IN 
PTR  
ns.skokie.com.sg.

15

IN
PTR
www.skokie.com.sg.

20

IN
PTR
mail.skokie.com.sg.

21

IN
PTR
po.skokie.com.sg.

db.127.0.0 File

;

;    File:      db.127.0.0 file

;    Purpose:   This file establishes the identity of this DNS.

;               SOA stands for 'start of authority' and sets the

;               default parameters for information this DNS is 

;               authoritative for:

;

@        IN SOA    ns.skokie.com.sg. postmaster.skokie.com.sg. (

        1997121901   ; serial  [yyyyMMddNN]

             21600   ; refresh [6h]

              3600   ; retry   [1h]

            691200   ; expire  [8d]

             86400)  ; minimum [1d]

;

         
IN 
NS 
ns.skokie.com.sg. 



IN
NS
secdns.pacific.net.sg.

1        
IN 
PTR   localhost.skokie.com.sg.

;

Scenario 6

Hosting Type 

: Multiple Domains for Mail Only




  Mail Servers on MULTIPLE hosts ONLY

Domains 

: skokie.com.sg




  ohare.com.sg




  palatine.com.sg

IP Range 

: 202.42.220.0 – 202.42.220.255

DNS Server Function : Primary DNS

Secondary DNS 
: secdns.pacific.net.sg

Gateway 


: gw.skokie.com.sg 
- 202.42.220.1

Name Server


: ns.skokie.com.sg
- 202.42.220.5

Web Server


: www.skokie.com.sg
- 202.42.220.15

Mail Server


: mail.skokie.com.sg
- 202.42.220.20

Secondary Mail Server
: po.skokie.com.sg
- 202.42.220.21

Mail Server – Ohare

: mail.ohare.com.sg 
- 202.42.220.40

Mail Server – palatine

: mail.palatine.com.sg
- 202.42.220.41

named.boot File

;

;    File:       named.boot

;    Purpose:    give the DNS its startup parameters and

;                list of startup files.

Directory c:\\bind

;

;check-names primary fail

;check-names secondary warn

;check-names response ignore

;

;

;    establish a loopback entry for this machine, and tell

;    it to load its identity from db.127.0.0

primary 0.0.127.IN-ADDR.ARPA db.127.0.0

;    XFRNETS parameter limits the transfer of zone information

;    to machines matching the subnet wildcard/mask entries listed.

;    WARNING: I have also added myself so that I can help test out

;             peoples configs that are having problems.

XFRNETS 199.72.93.0 127.0.0.0 202.42.220.0

;    set ourselves as primary server for the zone

primary skokie.com.sg db.zoneinfo

primary ohare.com.sg db.ohare

primary palatine.com.sg db.palatine

;    provide reverse address-to-host mapping

primary 220.42.202.in-addr.arpa db.202.42.220.0

;

; prime the DNS with root server 'hint' information

cache . db.cache

db.zoneinfo File

;

;    File:      db.zoneinfo

;    Purpose:   This file establishes the name/address information

;               for this zone.  You will have to fill out the actual

;               information for your specific zone in the format shown

;               in the comments.

;

@        IN SOA    ns.skokie.com.sg. postmaster.skokie.com.sg. (

        1997121901   ; serial  [yyyyMMddNN]

             21600   ; refresh [6h]

              3600   ; retry   [1h]

            691200   ; expire  [8d]

             86400)  ; minimum [1d]

skokie.com.sg
IN 
NS  
ns.skokie.com.sg. 




IN
NS
secdns.pacific.net.sg.

skokie.com.sg
IN
MX
10 mail.skokie.com.sg.




IN
A
202.42.220.20




IN
MX
20 po.skokie.com.sg.




IN
A
202.42.220.21

;
Define local hosts    

gw


IN
A
202.42.220.1

ns     

IN    A   
202.42.220.5

www


IN
A
202.42.220.15

mail


IN
A
202.42.220.20

po


IN
A
202.42.220.21

db.ohare File

;

;    File:      db.ohare

;    Purpose:   This file establishes the name/address information

;               for this zone.  You will have to fill out the actual

;               information for your specific zone in the format shown

;               in the comments.

;

@        IN SOA    ns.skokie.com.sg. postmaster.skokie.com.sg. (

        1997121901   ; serial  [yyyyMMddNN]

             21600   ; refresh [6h]

              3600   ; retry   [1h]

            691200   ; expire  [8d]

             86400)  ; minimum [1d]

ohare.com.sg
IN 
NS  
ns.skokie.com.sg. 




IN
NS
secdns.pacific.net.sg.

ohare.com.sg
IN
MX
10 mail.ohare.com.sg.




IN
A
202.42.220.40

;
Define local hosts    

mail


IN
A
202.42.220.40

db.palatine File

;

;    File:      db.palatine

;    Purpose:   This file establishes the name/address information

;               for this zone.  You will have to fill out the actual

;               information for your specific zone in the format shown

;               in the comments.

;

@        IN SOA    ns.skokie.com.sg. postmaster.skokie.com.sg. (

        1997121901   ; serial  [yyyyMMddNN]

             21600   ; refresh [6h]

              3600   ; retry   [1h]

            691200   ; expire  [8d]

             86400)  ; minimum [1d]

palatine.com.sg
IN 
NS  
ns.skokie.com.sg. 




IN
NS
secdns.pacific.net.sg.

palatine.com.sg
IN 
MX  
mail.palatine.com.sg. 




IN
A
202.42.220.41

;
Define local hosts    

mail


IN
A
202.42.220.41

db.202.42.220.0 File

;

;    File:      db.inaddr

;    Purpose:   This file establishes the address-to-name lookup

;               information for this zone.  You will have to

;               fill out the actual address information for your

;               specific zone in the format shown in the comments

;

@        IN SOA ns.skokie.com.sg. postmaster.skokie.com.sg. (

        1997121901   ; serial  [yyyyMMddNN]

             21600   ; refresh [6h]

              3600   ; retry   [1h]

            691200   ; expire  [8d]

             86400)  ; minimum [1d]

   
IN 
NS 
ns.skokie.com.sg. 


IN
NS
secdns.pacific.net.sg.

1        
IN 
PTR   gw.skokie.com.sg.

5       
IN 
PTR  
ns.skokie.com.sg.

15

IN
PTR
www.skokie.com.sg.

20

IN
PTR
mail.skokie.com.sg.

21

IN
PTR
po.skokie.com.sg.

40

IN
PTR
mail.ohare.com.sg.

41

IN
PTR
mail.palatine.com.sg.

db.127.0.0 File

;

;    File:      db.127.0.0 file

;    Purpose:   This file establishes the identity of this DNS.

;               SOA stands for 'start of authority' and sets the

;               default parameters for information this DNS is 

;               authoritative for:

;

@        IN SOA    ns.skokie.com.sg. postmaster.skokie.com.sg. (

        1997121901   ; serial  [yyyyMMddNN]

             21600   ; refresh [6h]

              3600   ; retry   [1h]

            691200   ; expire  [8d]

             86400)  ; minimum [1d]

;

         
IN 
NS 
ns.skokie.com.sg. 



IN
NS
secdns.pacific.net.sg.

1        
IN 
PTR   localhost.skokie.com.sg.

;

